4in6

4in6 is a method to transmit IPv4 traffic over explicit IPv6 connections.

It is achieved by using tunneling to encapsulate IPv4 traffic over configured IPv6 tunnels as defined in RFC 2473.

These tunnels are usually manually configured but they can be automated using protocols such as TSP.