ADPCM

Adaptive Differential Pulse-Code Modulation (ADPCM) is a differential pulse-code modulation variant where the size of quantization ranges is modified with a scaling factor before encoding. This means that the bandwidth requirements are reduced.