PTM Priority

The PTM Proprity defines how PTM traffic packets should be handled.

Priority	Description
Normal Priority	Send packets according to their priority.
High Priority	Use preemption; lower-priority packets are paused when higher-priority packets are sent.