Neighbor Solicitation

Neighbor solicitations are NDP discovery messages used to determine if a network neighbor is available at a cached address, or else request the actual network address.

In NDP, Neighbor Solicitation packets have the type 135.