Precedence

The Precedence setting defines quality of service parameters relating to Class Selector and Assured Forwarding priority.

ID	Setting
All	Default
0	CS1, AF11, AF12
1	CS2, AF21, AF22
2	CS3, AF31, AF32
3	CS4, AF41, AF42
4	CS5, Voice-admit, EF
5	CS5
6	CS6
7	CS7