RFC 5572

RFC 5572 discusses using TSP to set up IP tunnels with inner protocols, such as IPv6 or IPv4, inside various outer protocols packets, such as IPv4, IPv6, or UDP over IPv4 for IPv4 NAT traversal.

More information

https://tools.ietf.org/html/rfc2275