VPI

A Virtual Path Identifier - VPI, is used together with VCIs to enable ATM networks.

In an ATM network, each circuit is given a virtual channel identifier, and and each path is given a virtual path identifier.

The VCI identifies circuit/channel in use, and VPI matches the appropriate path to the desired destination host.